**COMMERCIAL PROPOSAL**

|  |  |
| --- | --- |
| Company Name | “Samarkand Automobile Factory” LLC |
| Brief information about the company | Our organization was established in 1999 in Samarkand city. In Tashkent city there is a representative office. To date, the company employs 983 people. |
| Company’s logo | \\Urmanov\фотосессия\_Сайт\Logo\Logo red horizontal.png |
| Address | Samarkand city, Bukhoriy street, 5 |
| CEO Name | Yuldashev Ulmas |
| Phone number | (+9971) 140 64 64, (+99871) 141 87 00, (+99866) 230 87 00 |
| Fax | (+99866) 2223839 |
| E-mail | info@samauto.uz, saminfo@samauto.uz |
| Web-site | www.samauto.uz |
| Products Produced | City and suburban buses (M3 categories of class I, II, III), medium and heavy-duty trucks (categories N2 and N3), specialized equipment: ambulance cars, fire trucks, etc. |
| Products quality parameters | Buses: Length - from 7 to 8 meters, Passenger capacity - from 32 to 56 people;  Trucks: Carrying capacity from 2 to 8 tons |
| Production volume | 4 000 units per year |
| Quality certificates | ISO 9001:2015, ISO 14001:2015, OHSAS 18001:2007, ISO 50001:2011 |
| Packaging |  |
| Price (USD / unit) | According to the price list (Appendix #1) |
| Delivery conditions |  |
| Product photos | \\Urmanov\фотосессия\_Сайт\Products\Bus\City\SAZ LE 60\SAZ LE 60 _.png \\Urmanov\фотосессия\_Сайт\Products\Bus\City\SAZ NP 37\SAZ NP 37 _.png  \\Urmanov\фотосессия\_Сайт\Products\Bus\Intercity bus\SAZ HD 50\SAZ HD 50 _.png \\Urmanov\фотосессия\_Сайт\Products\Bus\Intercity bus\SAZ NP 21\SAZ NP 21 _.png  \\Urmanov\фотосессия\_Сайт\Products\Bus\Intercity bus\SAZ NP 26\SAZ NP 26 _.png \\Urmanov\фотосессия\_Сайт\Products\Special body trucks\Ambulance\Ambulance.png  \\Urmanov\фотосессия\_Сайт\Products\Special body trucks\Communal services trucks\NQR 71 PL _.png \\Urmanov\фотосессия\_Сайт\Products\Special body trucks\Fire-fighting trucks\FTR 33 HLX\fire-fighting.png  \\Urmanov\фотосессия\_Сайт\Products\Special body trucks\Fire-fighting trucks\NQR 71 PL\fire-fighting.png \\Urmanov\фотосессия\_Сайт\Products\Special body trucks\Garbage trucks\NPR 82 L\NPR 82 (CNG) - мусоровоз_.png  \\Urmanov\фотосессия\_Сайт\Products\Special body trucks\Garbage trucks\NQR 71 PL\NQR 71 PL - мусоровоз_.png \\Urmanov\фотосессия\_Сайт\Products\Special body trucks\Tank trucks\Sanitation truck\NQR 71 PL - ассенизатор_.png  \\Urmanov\фотосессия\_Сайт\Products\Special body trucks\Tank trucks\Water carrier\NQR 71 PL.png\\Urmanov\фотосессия\вышка.png\\Urmanov\фотосессия\_Сайт\Products\Trucks\Dump trucks\Dump truck FVR 33 GLD\FVR 33 G _ .png\\Urmanov\фотосессия\_Сайт\Products\Trucks\Dump trucks\Dump truck NQR 71 PL\NQR 71 PL - самосвал _.png  \\Urmanov\фотосессия\_Сайт\Products\Trucks\Onboard\Onboard + tent FVR 33 PLX\FVR 33 P - тентовый _.png\\Urmanov\фотосессия\_Сайт\Products\Trucks\Onboard\Onboard + tent NPR 82 L\NPR 82 (CNG) - тентовый _.png \\Urmanov\фотосессия\_Сайт\Products\Trucks\Onboard\Onboard + tent NQR 71 PL\NQR 71 PL - onboard _.png\\Urmanov\фотосессия\_Сайт\Products\Trucks\Onboard\Onboard NQR 71 PL\NQR 71 PL - onboard2 _.png  \\Urmanov\фотосессия\_Сайт\Products\Trucks\Vans\FVR 33 PLX\FVR 33 P - закрытый металлический _.png\\Urmanov\фотосессия\_Сайт\Products\Trucks\Vans\NKR 55 E2\NKR 55 E2 _.png  \\Urmanov\фотосессия\_Сайт\Products\Trucks\Vans\NPR 82 L\NPR 82 L _.png\\Urmanov\фотосессия\_Сайт\Products\Trucks\Vans\NQR 71 PL\NQR 71 PL - закрытый металлический _.png  \\Urmanov\фотосессия\_Сайт\Products\Trucks\Vans\Refrigerator NQR\NQR 71 PL.png |

Appendix #1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Price-list of «Samarkand Automobile Factory» LLC** | | | | | |
| **№** | **Product name** | **Model** | **Performance specification** | **\* Unit Price**  **EXW-Samarkand, USD** | **Photo** |
| 1 | City Low Entry Bus | **SAZ LE 60** | Overall dimensions (L/W/H) – 8065/2470/2750 mm  Passengers capacity – 56 persons  Passenger seats – 25 persons  Gross vehicle weight (GVW) – 10 200 kg  Engine model – ISUZU 4HK1-TCC, diesel, Euro 4-5  Maximum power – 185 hp/130 kW(2600 rpm)  Vehicle control type: Left hand drive | 75 000 | Копия LE60 |
| 2 | Intercity bus | **SAZ HD 50** | Overall dimensions (L/W/H) – 8010/2320/2800 mm  Passengers capacity – 44 persons  Passenger seats – 29 persons  Gross vehicle weight (GVW) – 9 500 kg  Engine model – ISUZU 4HK1-TCN, diesel, Euro 4-5  Maximum power – 140 hp/109 kW(2600 rpm)  Vehicle control type: Left hand drive | 63 000 | C:\Users\fayzullo.SAF\Desktop\HD50 - little.jpg |
| 3 | Intercity bus (CNG) | **SAZ HC45** | Passengers capacity - 32 persons  Passenger seats – 18 persons  Overall dimensions (L/W/H) – 7100х2250х2880mm  Gross vehicle weight (GVW) – 7 500 kg  Engine model – ISUZU 4HV1 CNG, Euro-4  Maximum power – 130 л.hp/96 kW (3200 rpm)  Ёмкость топливных баков 2 шт – 30/30 м3 =60 м3 | 50 000 | vyrezat |
| 4 | City Bus | **SAZ HD 41** | Overall dimensions (L/W/H) – 6920х2240х2880 mm  Passengers capacity – 45 persons  Passenger seats – 17 persons  Engine model – ISUZU 4HG1, diesel, Euro 3  Maximum power – 121 hp/89 kW (3200 rpm)  Vehicle control type: Left hand drive | 37 000 | NP37_сбоку |
| 5 | City Bus | **SAZ HC 40** | Overall dimensions (L/W/H): 6920 / 2240 / 2880 mm  Passengers capacity – 38 persons  Passenger seats – 16 persons  Engine model – ISUZU 4HF1, diesel, Euro 2  Maximum power – 104 hp/78 kW(3200 rpm)  Vehicle control type: Left hand drive | 31 500 | NP37_сбоку |
| 6 | Intercity bus | **SAZ NP 26** | Overall dimensions (L/W/H): 6920 / 2240 / 2880 mm  Passengers capacity – 26 persons   * passenger – 24 seats * crew – 2 seats   Engine model – ISUZU 4HF1, diesel, Euro 2  Maximum power – 104 hp /78 kW(3200 rpm)  Vehicle control type: Left hand drive | 33 000 | NP26 |
| 7 | Intercity bus | **SAZ NP 21** | Overall dimensions (L/W/H): 6920 / 2240 / 2880 mm  Passengers capacity – 21 persons   * passenger – 20 seats * crew – 2 seats   Engine model – ISUZU 4HF1, diesel, Euro 2  Maximum power – 104 hp /78 kW(3200 rpm)  Vehicle control type: Left hand drive | 33 000 | np21_ |
| 8 | Van | **ISUZU**  **NPR82 (CNG)** | Overall dimensions (L/W/H) – 6795 / 2300 / 3000 mm  Payload – 3550 kg  Engine model – ISUZU 4HV1, Euro 4  Maximum power – 131 hp /96 kW(3200 rpm)  Fuel type – compressed natural gas (CNG)  Vehicle control type: Left hand drive | 37 500 | Без именийц-2 |
| 9 | Cargo tent truck | **ISUZU**  **NPR82 (CNG)** | Overall dimensions (L/W/H)– 6795 / 2300 / 3000 mm  Payload – 3550 kg  Engine model – ISUZU 4HV1, Euro 4  Maximum power – 131 hp /96 kW(3200 rpm)  Fuel type– compressed natural gas (CNG)  Vehicle control type: Left hand drive | 37 000 | 555555556 |
| 10 | Garbage truck | **ISUZU**  **NPR82 (CNG)** | Overall dimensions (L/W/H)– 7300 / 2240 / 2840 mm  Payload – 1140 kg  Body space – 7 mc  Engine model – ISUZU 4HV1, Euro 4  Maximum power – 131 hp /96 kW(3200 rpm)  Fuel type– compressed natural gas (CNG) | 54 000 | мусоровоз CNG (mall size) |
| 11 | Dump truck | **ISUZU**  **NPR82 (CNG)** | Overall dimensions (L/W/H) – 6214 / 2150 / 2454 mm  Payload – 4000 kg  Engine model – ISUZU 4HV1, Euro 4  Maximum power – 121 hp /89 kW(3200 rpm)  Fuel type– compressed natural gas (CNG)  Vehicle control type: Left hand drive | 45 000 | Самосвал - копия |
| 12 | Cesspool cleaner | **ISUZU NPR82 (CNG)** | Overall dimensions (L/W/H) – 7060 / 1665 / 2560 mm  Tank volume – 4120 l,  Engine model – ISUZU 4HV1, diesel, Euro 4  Maximum power – 130 hp /96 kW(3200 rpm)  Fuel type– compressed natural gas (CNG)  Vehicle control type: Left hand drive | 44 700 | 23405864_1464211753698694_5066046427712756174_o |
| 13 | Chassis | **ISUZU**  **NKR 55E** | Overall dimensions (L/W/H) – 4610 / 1860 / 2120 mm  Gross vehicle weight – 5 200 kg  Chassis mass – 2 885 kg,  Engine model – ISUZU 4JB1, diesel, Euro 2  Maximum power – 80 hp /59 kW (3600 rpm)  Wheel base – 2 460 mm | 20 000 | C:\Users\fayzullo\Desktop\nkr.png |
| 14 | Van | **ISUZU**  **NKR 55E** | Overall dimensions (L/W/H) – 4730/ 1975 / 2750 mm  Payload – 2430 kg  Engine model – ISUZU 4JB1, diesel, Euro 2  Maximum power – 59 hp /80 kW(3600 rpm)  Vehicle control type: Left hand drive | 24 000 | nkr-1 |
| 15 | Isothermal van | **ISUZU**  **NKR 55E** | Payload – 2430 kg  Engine model – ISUZU 4JB1, diesel, Euro 2  Overall dimensions (L/W/H) – 4730/ 1975 / 2750 mm  Maximum power – 59 hp /80 kW(3600 rpm)  Vehicle control type: Left hand drive | 27 000 | nkr-1 |
| 16 | Refrigerated van | **ISUZU**  **NKR 55E** | Overall dimensions (L/W/H) – 4730/1975/2750 mm  Payload – 2350 kg, Body space – 14 mc  Cooling temperature – (+5С⁰ ÷ -5С⁰) / (0С⁰ ÷ -18С⁰)  Engine model – – ISUZU 4JB1, diesel, Euro 2  Maximum power – 80 hp /59 kW (3600 rpm)  Wheel base – 2 460 mm | 30 000 | nkr-1 |
| 17 | Ambulance | **ISUZU**  **NKR 55E** | Overall dimensions (L/W/H) – 5110 / 1950 / 2660 mm  Gross vehicle weight – 5 200 kg  Engine model – ISUZU 4JB1, diesel, Euro 2  Maximum power – 80 hp /59 kW (3600 rpm)  Wheel base – 2 460 mm | 57 000 | **Шер517** |
| 18 | Chassis | **ISUZU NMR 77H**  **(Euro 3)** | Overall dimensions (L/W/H)- 4730х1815х2160 mm,  Gross vehicle weight – 5 200 kg  Engine model – ISUZU 4JH1-TC, diesel, Euro 3  Maximum power – 96 hp /106 kW (3200 rpm)  Breaking system – drum type with ABS | 22 500 | **isuzu_elf35** |
| 19 | Chassis | **ISUZU NMR 85H**  **(Euro 5)** | Overall dimensions (L/W/H)- 6110х1815х2160 mm,  Gross vehicle weight – 5 500 kg, Chassis weight– 2 295 kg  Engine model – ISUZU 4JJ1-TCC, diesel, Euro 5  Maximum power – 91 hp /124 kW (2800 rpm)  Breaking system – drum type with ABS  Fuel tank capacity -75 l | 27 000 | **isuzu_elf35** |
| 20 | Chassis | **ISUZU NMR 85E**  **(Euro 5)** | Overall dimensions (L/W/H)- 6110х1815х2160 mm,  Gross vehicle weight – 5 500 kg ,Chassis weight– 2 000 kg  Engine model – ISUZU 4JJ1-TCC, diesel, Euro 5  Maximum power – 91 hp /124 kW (2800 rpm)  Breaking system – drum type with ABS  Fuel tank capacity -100 l | 27 000 | **isuzu_elf35** |
| 21 | Chassis | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6610 / 1995 / 2250 mm  Payload – 5570 kg  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm) | 23 000 | gruzovik N-xxx |
| 22 | Chassis | **ISUZU**  **NPR 75L-K**  **(Euro 3)** | Overall dimensions (L/W/H)- 6635х2040х2255 mm,  Gross vehicle weight – 7 500 kg ,Chassis weight– 2 705 kg  Engine model – ISUZU 4HK1-TCN, diesel, Euro 3  Maximum power – 110 hp /150 kW (2600 rpm)  Breaking system – drum type with ABS  Fuel tank capacity -100 l | 25 000 |  |
| 23 | Chassis | **ISUZU**  **NPR 75L-K (Euro 5)** | Overall dimensions (L/W/H)- 6635х2040х2255 mm,  Gross vehicle weight – 7 500 kg ,Chassis weight– 2 705 kg  Engine model – ISUZU 4HK1-TCN, diesel, Euro 5  Maximum power – 110 hp /150 kW (2600 rpm)  Breaking system – drum type with ABS  Fuel tank capacity -100 l | 30 500 |  |
| 24 | Lorry with sides | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6730 / 2210 / 3098 mm  Payload – 3755 kg,  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Wheel base – 2 460 mm  Vehicle control type: Left hand drive | 27 500 | b3ff2ea76dfbae66c3dab53b7b5cee4a |
| 25 | Cargo tent truck | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6730 / 2300 / 3098 mm  Payload – 3755 kg, Body space – 20 mc  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 29 000 | тентовый NQR2 |
| 26 | Van | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6730 / 2210 / 3098 mm  Payload – 3995 kg, Body space – 20 mc  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 29 000 | фургон NQR2 |
| 27 | Refrigerated van | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6730 / 2240 / 3098 mm  Payload – 3000 kg, Body space – 19 mc  Cooling temperature – (+5С⁰ ÷ -5С⁰) / (0С⁰ ÷ -18С⁰)  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 38 000 | рефрижератор NQR |
| 28 | Beverages van | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6580 / 2200 / 2720 mm  Payload – 4200 kg, Body capacity – 6 pallets  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 31 000 | напитковоз N-1 |
| 29 | Bakery van | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6455 / 2234 / 2250 mm  Payload – 3945 kg  Tray for bakery – 140 trays  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 31 000 | хлебовоз NQR |
| 30 | Dump truck | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6214 / 2150 / 2454 mm  Payload – 4000 kg  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 35 000 | Самосвал-1 |
| 31 | Garbage truck | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 7130 / 2240 / 2700 mm  Payload – 2020 kg, Body cubic capacity – 7 mc  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 44 000 | мусоровоз NQR |
| 32 | Water carrier | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6700 / 2180 / 2560 mm  Tank volume – 4170 l,  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 33 000 | Water-1 |
| 33 | Cesspool cleaner | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 7060 / 1665 / 2560 mm  Tank volume – 4120 l,  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 33 000 |  |
| 34 | Breakdown truck | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 7060х1665х2560 mm  Payload – 4 400 kg,  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Wheel base – 2 460 mm  Vehicle control type: Left hand drive | 43 000 |  |
| 35 | Milk tanker | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 7060 / 1665 / 2560 mm  Tank volume – 4000 l,  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 42 000 |  |
| 36 | Street washer | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 7060 / 1665 / 2560 mm  Tank volume – 4120 l,  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Wheel base – 2 460 mm  Vehicle control type: Left hand drive | 41  000 | 258-1 - копия |
| 37 | Fire-fighting vehicle | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6870 / 2150 / 2480 mm  Water tank volume – 1700 liter  Foam tank volume – 150 liter  Engine model –ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm)  Vehicle control type: Left hand drive | 152 000 | пожар |
| 38 | Telescopic tower | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 7047 / 1995 / 3360 mm,  Basket payload – 250 kg,  Maximum working height – 22m  Engine model –ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm) | 79 500 | C:\Users\fayzullo.SAF\Desktop\вышка NQR-1.jpg |
| 39 | Telescopic tower | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 7047 / 1995 / 3360 mm,  Basket payload – 200 kg,  Maximum working height – 18m  Engine model –ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm) | 72 900 | C:\Users\fayzullo.SAF\Desktop\вышка NQR-1.jpg |
| 40 | Vacuum cleaning sweeper | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 6730 / 2210 / 2350 mm,  Water tank volume – 800 liter,  Body cubic capacity – 4 mc  Engine model –ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm) | 107 000 | Пылесос N-1 |
| 41 | Crane manipulator | **ISUZU**  **NQR 71 PL** | Overall dimensions (L/W/H) – 6730х2300х2380 mm  Lifting capacity – 3200 kg  Maximum lift height – 12 m  Maximum working radius – 9,45 m  Engine model – ISUZU 4HG1, diesel, Euro 2  Maximum power – 121 hp /89 kW(3200 rpm) | 50 000 | 07-1 |
| 42 | Evacuator with a crane (up to 8.4 m - 1.5 tons) | **ISUZU**  **NQR 71PL** | Overall dimensions (L/W/H) – 7060х1665х2560 мм  Lifting capacity – 4400 кг  Tractive force of winch - 3500 kg  Engine - ISUZU 4HG1, diesel, Euro-2  Engine power - 121 HP / 89 kW at 3200 rpm | 72 500 | эвакуатор-1 (2) |
| 43 | Chassis | **ISUZU**  **FTR 33 HLX** | Overall dimensions (L/W/H) – 7420 / 2400 / 2570 mm  Gross vehicle weight – 13 300 kg  Chassis mass – 4780 kg,  Engine model – ISUZU 6HH1-S, diesel, Euro 1  Maximum power – 200 hp / 147 kW (2 850 rpm)  Wheel base – 3650 mm  Fuel tank capacity – 200 liter | 31 000 | shassi F |
| 44 | Chassis | **ISUZU**  **FTR 34L-E**  **(Euro 3)** | Overall dimensions (L/W/H)- 7665х2450х2860 mm,  Wheel arrangement - 4 х 2 / rear (dual)  Wheel base – 4 250 mm, Gross vehicle weight – 14 200 kg  Engine model – ISUZU 6HK1-TCN, diesel, Euro 3  Maximum power – 177 hp /240 kW (2400 rpm)  Transmission - ISUZU MZW6P, manual control  Breaking system – drum type with ABS  Fuel tank capacity – 200 liter | 39 000 | 62 |
| 45 | Chassis | **ISUZU**  **FVR 33 GLD** | Overall dimensions (L/W/H) – 6770 / 2465 / 2670 mm  Gross vehicle weight – 15 100 kg  Chassis mass – 4880 kg,  Engine model – ISUZU 6HH1-S, diesel, Euro 1  Maximum power – 200 hp / 147 kW (2 850 rpm)  Wheel arrangement 4х2 / rear  Wheel base – 3 900 mm | 36 000 | shassi F |
| 46 | Chassis | **ISUZU**  **FVR 34K-E**  **(Euro 3)** | Overall dimensions (L/W/H) - 6755х2460х2900 mm  Wheel base – 3 900 mm, Gross vehicle weight – 17 000 kg  Engine model – ISUZU 6HK1-TCN, diesel, Euro 3  Maximum power – 177 hp /240 kW (2400 rpm)  Transmission - ISUZU MZW6P, manual control  Breaking system – drum type with ABS  Fuel tank capacity – 200 liter | 41 000 | 62 |
| 47 | Chassis | **ISUZU**  **FVR 33 PLX** | Overall dimensions (L/W/H) – 9270 / 2465 / 2670 mm  Gross vehicle weight – 15 100 kg  Chassis mass – 5130 kg,  Engine model – ISUZU 6HH1-S, diesel, Euro I  Maximum power – 200 hp / 147 kW (2 850 rpm)  Wheel arrangement 4х2 / rear  Wheel base – 5 550 mm  Fuel tank capacity – 200 liter | 37 000 | shassi F |
| 48 | Chassis | **ISUZU**  **FVR 34M-E**  **(Euro 3)** | Overall dimensions (L/W/H) - 7955х2459х2885 mm  Wheel arrangement - 4 х 2 / rear (dual)  Wheel base – 4 650 mm, Gross vehicle weight – 17 000 kg  Engine model – ISUZU 6HK1-TCN, diesel, Euro 3  Maximum power – 221 hp /300 kW (2400 rpm)  Transmission - ZF9S1110, manual control  Breaking system – drum type with ABS  Fuel tank capacity – 200 liter | 54 500 | 62 |
| 49 | Chassis | **ISUZU**  **FVR 34Q-E**  **(Euro 3)** | Overall dimensions (L/W/H) - 9255х2459х2885 мм,  Wheel arrangement - 4 х 2 / rear (dual)  Wheel base – 5 550 mm, Gross vehicle weight – 17 000 kg  Engine model – ISUZU 6HK1-TCN, diesel, Euro 3  Maximum power – 177 hp /240 kW (2400 rpm)  Transmission - ISUZU MZW6P, manual control  Breaking system – drum type with ABS  Fuel tank capacity – 200 liter | 41 000 | 62 |
| 50 | Lorry with sides | **ISUZU**  **FVR 33 PLX** | Overall dimensions (L/W/H) – 9270 / 2465 / 2670 mm  Payload – 8000 kg  Engine model – ISUZU 6HH1-S, diesel, Euro I  Maximum power – 200 hp / 147 kW (2 850 rpm)  Wheel arrangement 4х2 / rear  Fuel tank capacity – 200 liter | 47 000 |  |
| 51 | Cargo tent truck | **ISUZU**  **FVR 33 PLX** | Overall dimensions (L/W/H) – 9330 / 2490 / 3490 mm  Payload – 7785 kg, Body space – 32 mc  Engine model – ISUZU 6HH1-S, diesel, Euro I  Maximum power – 200 hp / 147 kW (2 850 rpm)  Wheel arrangement 4х2 / rear  Fuel tank capacity – 200 liter | 47 700 | тентовый FVR |
| 52 | Van | **ISUZU**  **FVR 33 PLX** | Overall dimensions (L/W/H) – 9300 / 2490 / 3400 mm  Payload – 7580 kg, Body space – 33 mc  Engine model – ISUZU 6HH1-S, diesel, Euro I  Maximum power – 200 hp / 147 kW (2 850 rpm)  Wheel arrangement 4х2 / rear  Fuel tank capacity – 200 liter | 48 000 | фургон FVR1 |
| 53 | Garbage truck | **ISUZU**  **FVR 33GLD** | Overall dimensions (L/W/H) – 8100 / 2450 / 2850 mm  Payload – 6250 kg, Body cubic capacity – 10+1.5 mc  Engine model – ISUZU 6HH1-S, diesel, Euro 1  Maximum power – 200 hp /147 kW(2850 rpm)  Fuel tank capacity – 200 liter | 65 000 | Мусоровоз F_white+isuzu |
| 54 | Dump truck | **ISUZU**  **FVR 33GLD** | Overall dimensions (L/W/H) – 6500 / 2490 / 2950 mm  Payload – 8000 kg  Engine model – ISUZU 6HH1-S, diesel, Euro I  Maximum power – 200 hp /147 kW(2850 rpm)  Fuel tank capacity – 200 liter | 55 000 | самосвал F |
| 55 | Street sweeper | **ISUZU**  **FVR 33 GLD** | Overall dimensions (L/W/H) – 8250 / 2900 / 2960 mm  Water tank volume – 7,4 mc  Engine model – ISUZU 6HH1-S, diesel, Euro I  Maximum power – 200 hp / 147 kW (2 850 rpm)  Working width, m   * washing/watering – 8 / 18 m * sweeping/cleaning – 2.3 m | 83 000 | КДМ Крантас |
| 56 | Water carrier | **ISUZU**  **FVR 33 GLD** | Overall dimensions (L/W/H) – 8250х2900х2960 мм  Gross vehicle weight – 15 100 kg, Tank volume – 8 mc  Engine model – ISUZU 6HH1-S, diesel, Euro 1  Maximum power – 200 hp / 147 kW (2 850 rpm)  Fuel tank capacity – 200 liter | 61 000 | Водовоз 8 м3 co |
| 57 | Truck crane | **ISUZU**  **FVR 33GLD** | Overall dimensions (L/W/H) – 8250х2900х2960 мм  Gross vehicle weight – 15 100 kg  Lifting capacity – 16 t  Engine model – ISUZU 6HH1-S, diesel, Euro 1  Maximum power – 200 hp / 147 kW (2 850 rpm)  Fuel tank capacity – 200 liter | 103 000 | 87501 |
| 58 | Fuel tanker  (with pump and ТРК) | **ISUZU**  **FVR 34K-E**  **(Euro 3)** | Overall dimensions (L/W/H) – 8 000х2500х3000 mm  Tanker dimensions (L/W/H) – 4000х2300х2000 mm  Tanker volume – 8 mc  Engine model – ISUZU 6HK1-TCN, diesel, Euro 3  Maximum power – 240 hp /177 kW (2400 rpm)  Fuel tank capacity – 200 liter | 69 000 | Бензовоз 8м3 |
| 59 | Fire-fighting vehicle | **ISUZU**  **FTR 33HLX** | Overall dimensions (L/W/H) – 7750 / 2800 / 3232 mm  Water tank volume – 4000 liter  Foam tank volume – 400 liter  Engine model – ISUZU 6HH1-S, diesel, Euro I  Maximum power – 200 hp /147 kW (2850 rpm) | 167 000 | пожарка FTR1 |
| 60 | Fire-fighting vehicle | **ISUZU**  **FVR 23K** | Overall dimensions (L/W/H) – 8340х2570х3250 mm  Water tank volume – 6000 liter  Foam tank volume – 600 liter  Engine model – ISUZU 6SD1, diesel, Euro 1  Maximum power – 240 hp /177 kW (2500 rpm)  Fuel tank capacity – 200 liter | 194 000 | пожарка FTR1 |
| 61 | Vacuum cleaning sweeper | **ISUZU**  **FTR 33HLX** | Overall dimensions (L/W/H) – 7420 / 2400 / 2570 mm  Water tank volume – 1100 liter  Dustbin capacity - 4 mc  Working surface – 2200 mm.  Engine model – ISUZU 6HH1-S, diesel, Euro I  Maximum power – 200 hp /147 kW (2850 rpm) | 125 700 | FTR 33 H - ваакумная подмитально-уборочная машина_ |
| 62 | Dump truck | **ISUZU**  **CYZ 51P** | Overall dimensions (L/W/H) – 8540х2515х3520 mm  Payload – 20 t  Wheel arrangement – 6х4  Погрузочная высота кузова – 2580 мм,  Engine model – ISUZU 6WF1-TCC, diesel, Euro 2,  Maximum power – 390 hp /287 kW (1800 rpm)  Fuel tank capacity – 400 liter | 91 000 | D:\EXPORT SECTION\ДИСТРИБЬЮТОР\Туркменистан\Тендер самосвал\ceseries-5.jpg |
| 63 | Шасси  грузового автомобиля | **ISUZU**  **NPS 75H**  **(Евро-3)** | Габаритные размеры (ДхШхВ) - 6635х2040х2255 мм,  Полная масса – 6 000 кг, Масса шасси – 2 910 кг,  Двигатель – ISUZU 4HK1-TCN, дизель, Евро-3  Мощность двигателя – 110 кВт/ 150 л.с. (2600 об/мин)  Рабочий объем цилиндров - 5193 см3  Тормозная система – барабанный, с ABS  Ёмкость топливного бака 100 л  Колесная формула – 4х4 | 38 000 |  |
| 64 | Chassis | **ISUZU**  **NPR82 (CNG)** | Overall dimensions (L/W/H) – 6635 / 2115 / 2270 mm  Gross vehicle weight – 7 500 kg  Chassis mass – 2 885 kg,  Engine model – ISUZU 4HV1, Euro 4  Maximum power – 131 hp /96 kW(3200 rpm)  Wheel arrangement 4х2 / rear  Wheel base – 3 845 mm  Fuel type – compressed natural gas (CNG) | 33 500 | C:\Users\fayzullo\Desktop\IMG_5042.jpg |

* ***All prices are performed on FCA basis- LLC “Samarkand Automobile Factory”, Samarkand, Uzbekistan on standard option models for a month after publication from 09/07/2018.***